../Core/Src/w25qxx.c:46:9:W25qxx_Spi	32	static
../Core/Src/w25qxx.c:54:10:W25qxx_ReadID	24	static
../Core/Src/w25qxx.c:67:6:W25qxx_ReadUniqID	24	static
../Core/Src/w25qxx.c:78:6:W25qxx_WriteEnable	8	static
../Core/Src/w25qxx.c:86:6:W25qxx_WriteDisable	8	static
../Core/Src/w25qxx.c:94:9:W25qxx_ReadStatusRegister	24	static
../Core/Src/w25qxx.c:120:6:W25qxx_WriteStatusRegister	16	static
../Core/Src/w25qxx.c:142:6:W25qxx_WaitForWriteEnd	8	static
../Core/Src/w25qxx.c:164:6:W25qxx_Init	16	static
../Core/Src/w25qxx.c:311:6:W25qxx_EraseChip	8	static
../Core/Src/w25qxx.c:334:6:W25qxx_EraseSector	16	static
../Core/Src/w25qxx.c:363:6:W25qxx_EraseBlock	16	static
../Core/Src/w25qxx.c:393:10:W25qxx_PageToSector	16	static
../Core/Src/w25qxx.c:398:10:W25qxx_PageToBlock	16	static
../Core/Src/w25qxx.c:403:10:W25qxx_SectorToBlock	16	static
../Core/Src/w25qxx.c:408:10:W25qxx_SectorToPage	16	static
../Core/Src/w25qxx.c:413:10:W25qxx_BlockToPage	16	static
../Core/Src/w25qxx.c:418:7:W25qxx_IsEmptyPage	72	static
../Core/Src/w25qxx.c:487:7:W25qxx_IsEmptySector	72	static
../Core/Src/w25qxx.c:556:7:W25qxx_IsEmptyBlock	72	static
../Core/Src/w25qxx.c:625:6:W25qxx_WriteByte	16	static
../Core/Src/w25qxx.c:652:7:W25qxx_WritePage	24	static
../Core/Src/w25qxx.c:702:7:W25qxx_WriteSector	40	static
../Core/Src/w25qxx.c:745:7:W25qxx_WriteBlock	40	static
../Core/Src/w25qxx.c:784:7:W25qxx_ReadByte	16	static
../Core/Src/w25qxx.c:809:6:W25qxx_ReadBytes	24	static
../Core/Src/w25qxx.c:847:7:W25qxx_ReadPage	24	static
../Core/Src/w25qxx.c:891:7:W25qxx_ReadSector	40	static
../Core/Src/w25qxx.c:932:7:W25qxx_ReadBlock	40	static
../Core/Src/w25qxx.c:972:10:read_data_length	4	static
../Core/Src/w25qxx.c:982:10:read_rfid_data_length	4	static
../Core/Src/w25qxx.c:992:10:SFlash_read	32	static
../Core/Src/w25qxx.c:1036:10:SFlash_read_to_check	24	static
../Core/Src/w25qxx.c:1068:10:SFlash_rfid_read	32	static
../Core/Src/w25qxx.c:1103:6:SFlash_rfid_write	24	static
../Core/Src/w25qxx.c:1167:6:SFlash_write	24	static
../Core/Src/w25qxx.c:1230:6:SRfid_pointer_read	24	static
../Core/Src/w25qxx.c:1247:6:SFlash_pointer_read	24	static
../Core/Src/w25qxx.c:1264:6:SFlash_pointer_write	16	static
../Core/Src/w25qxx.c:1280:6:SRfid_pointer_write	16	static
../Core/Src/w25qxx.c:1296:6:rvereseArray	32	static
../Core/Src/w25qxx.c:1309:9:read_last_data	40	static
../Core/Src/w25qxx.c:1353:9:read_rfid_last_data	40	static
